default -> -   (Coverage 10000, error 23.0%, error without exceptions 50.0%)
   unless ATA -> +   (Coverage 9941, error 22.8%, error without exceptions 50.0%)
      unless CCAAG -> -   (Coverage 5224, error 24.2)%
