default -> -   (Coverage 3000, error 22.3%, error without exceptions 50.0%)
   unless ATA -> +   (Coverage 2981, error 22.2%, error without exceptions 49.9%)
      unless CCAAG -> -   (Coverage 1603, error 24.2)%
