default -> -   (Coverage 7500, error 22.9%, error without exceptions 50.0%)
   unless ATA -> +   (Coverage 7463, error 22.8%, error without exceptions 49.9%)
      unless CCAAG -> -   (Coverage 3917, error 24.2)%
